,Nominal Diameter 1##PIPE_SIZE##INCHES,Nominal Diameter 2##PIPE_SIZE##INCHES,Maximum Working Pressure##PIPING_PRESSURE##POUNDS_FORCE_PER_SQUARE_INCH,Maximum Operating Temperature##HVAC_TEMPERATURE##FAHRENHEIT,Unit Weight##FORCE##POUNDS_FORCE,Model Number##OTHER##,Ring Material##OTHER##,Fitting Material##OTHER##,Description##OTHER##,Standards##OTHER##,Product Page URL##OTHER##,URL##OTHER##
0.375in.x0.5in. Copper Female,0.375,0.5,150,210,0.5,499860-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
0.5in.x0.5in. Copper Female,0.5,0.5,150,210,0.065,499794-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
0.5in.x0.75in. Copper Female,0.5,0.75,150,210,0.095,499793-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
0.625in.x0.75in. Copper Female,0.625,0.75,150,210,0.137,499862-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
0.75in.x0.75in. Copper Female,0.75,0.75,150,210,0.145,499797-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
0.75in.x1in. Copper Female,0.75,1,150,210,0.2,499798-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
1in.x1in. Copper Female,1,1,150,210,0.24,499800-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
1.25in.x1.25in. Copper Female,1.25,1.25,150,210,0.372,499802-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
1.5in.x1.5in. Copper Female,1.5,1.5,150,210,0.474,499804-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
2in.x2in. Copper Female,2,2,150,210,0.995,499806-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960,https://www.REHAU.com/
