,Nominal Diameter 1##PIPE_SIZE##INCHES,Nominal Diameter 2##PIPE_SIZE##INCHES,Maximum Working Pressure##PIPING_PRESSURE##POUNDS_FORCE_PER_SQUARE_INCH,Maximum Operating Temperature##HVAC_TEMPERATURE##FAHRENHEIT,Overall Length##LENGTH##FEET,Overall Height##LENGTH##FEET,Unit Weight##FORCE##POUNDS_FORCE,Model Number##OTHER##,Fitting Material##OTHER##,Ring Material##OTHER##,Description##OTHER##,Standards##OTHER##,Product Page URL##OTHER##
0.5in. x 0.5in. FPT,0.5,0.5,150,210,0.130833333,0.093333333,0.13,499821-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.5in. x 0.75in. FPT,0.5,0.75,150,210,0.145833333,0.110833333,0.19,499819-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.75in. x 0.75in. FPT,0.75,0.75,150,210,0.155833333,0.110833333,0.19,499822-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.75in. x 1in. FPT,0.75,1,150,210,0.184166667,0.14,0.375,499820-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1in. x 1in. FPT,1,1,150,210,0.203333333,0.14,0.41,499823-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1.25in. x 1.25in. FPT,1.25,1.25,150,210,0.215833333,0.173333333,0.548,499863-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1.5in. x 1.5in. FPT,1.5,1.5,150,210,0.249166667,0.198333333,0.809,499864-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
2in. x 2in. FPT,2,2,150,210,0.294166667,0.25,1.639,499866-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
