,Nominal Diameter 1##PIPE_SIZE##INCHES,Nominal Diameter 2##PIPE_SIZE##INCHES,Maximum Working Pressure##PIPING_PRESSURE##POUNDS_FORCE_PER_SQUARE_INCH,Maximum Operating Temperature##HVAC_TEMPERATURE##FAHRENHEIT,Overall Length##LENGTH##FEET,Overall Height##LENGTH##FEET,Unit Weight##FORCE##POUNDS_FORCE,Model Number##OTHER##,Ring Material##OTHER##,Fitting Material##OTHER##,Description##OTHER##,Standards##OTHER##,Product Page URL##OTHER##
0.375in.x0.5in. Copper Male,0.375,0.5,150,210,0.1075,0.056666667,0.035,499859-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.5in.x0.5in. Copper Male,0.5,0.5,150,210,0.1175,0.060833333,0.05,499795-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.5in.x0.75in. Copper Male,0.5,0.75,150,210,0.138333333,0.079166667,0.085,499790-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.625in.x0.75in. Copper Male,0.625,0.75,150,210,0.151666667,0.0775,0.9,499861-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.75in.x0.5in. Copper Male,0.75,0.5,150,210,0.1375,0.091666667,0.095,499792-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.75in.x0.75in. Copper Male,0.75,0.75,150,210,0.158333333,0.091666667,0.015,499796-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.75in.x1in. Copper Male,0.75,1,150,210,0.171666667,0.1,0.135,499791-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1in.x1in. Copper Male,1,1,150,210,0.190833333,0.115,0.195,499799-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1.25in.x1.25in. Copper Male,1.25,1.25,150,210,0.218333333,0.123333333,0.291,499801-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1.5in.x1.5in. Copper Male,1.5,1.5,150,210,0.25,0.145,0.414,499803-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
2in.x2in. Copper Male,2,2,150,210,0.318333333,0.2175,1.108,499805-001,Plastic - REHAU - Polyethylene - White,Metal - REHAU - LF Brass,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
