,Nominal Diameter 1##PIPE_SIZE##INCHES,Nominal Diameter 2##PIPE_SIZE##INCHES,Maximum Working Pressure##PIPING_PRESSURE##POUNDS_FORCE_PER_SQUARE_INCH,Maximum Operating Temperature##HVAC_TEMPERATURE##FAHRENHEIT,Overall Length##LENGTH##FEET,Overall Height##LENGTH##FEET,Unit Weight##FORCE##POUNDS_FORCE,Model Number##OTHER##,Fitting Material##OTHER##,Ring Material##OTHER##,Description##OTHER##,Standards##OTHER##,Product Page URL##OTHER##
0.5in. x 0.5in. MPT,0.5,0.5,150,210,0.144166667,0.081666667,0.115,499807-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.5in. x 0.75in. MPT,0.5,0.75,150,210,0.148333333,0.105833333,0.18,499810-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.75in. x 0.75in. MPT,0.75,0.75,150,210,0.168333333,0.105833333,0.19,499808-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
0.75in. x 1in. MPT,0.75,1,150,210,0.185,0.128333333,0.325,499814-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1in. x 0.75in. MPT,1,0.75,150,210,0.188333333,0.104166667,0.22,499809-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1in. x 1in. MPT,1,1,150,210,0.205,0.128333333,0.395,499815-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1.25in. x 1.25in. MPT,1.25,1.25,150,210,0.244166667,0.161666667,0.348,499816-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
1.5in. x 1.5in. MPT,1.5,1.5,150,210,0.283333333,0.180833333,0.864,499817-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
2in. x 2in. MPT,2,2,150,210,0.321666667,0.233333333,1.354,499818-001,Metal - REHAU - LF Brass,Plastic - REHAU - Polyethylene - White,LF Brass Adapter,CAN/CSA B137.5; ASTM F877; ASTM F1960,https://www.REHAU.com/us-en/mechanicalplumbing/search-by-product/REHAU-f1960
